---
title: sFlow configuration · Cloudflare Magic Network Monitoring docs
description: A step-by-step configuration guide for exporting sFlow data to
  Cloudflare's network.
lastUpdated: 2025-10-16T11:21:23.000Z
chatbotDeprioritize: false
source_url:
  html: https://developers.cloudflare.com/magic-network-monitoring/routers/sflow-config/
  md: https://developers.cloudflare.com/magic-network-monitoring/routers/sflow-config/index.md
---

1. Log in to your router's configuration application.

2. Open your router's sFlow configuration menu.

3. Set up your router's **sFlow Exporter** configuration with the following values:

   * **Destination IP address**: `162.159.65.1`
   * **Destination Port**: `6343`
   * **Transport Protocol**: `UDP`
